For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster bezel. Refer to Instrument Cluster Replacement in Instrument Panel, Gages and Console.
2. Disconnect the electrical connectors.
3. Release the retainer tabs using a small flat bladed tool.
4. Remove the switch.

### Installation Procedure

1. Install the headlamp switch and/or the panel dimmer switch to the bezel to the retainers.
2. Connect the electrical connectors to the switch.
3. Install the bezel to the instrument panel. Refer to Instrument Cluster Replacement in Instrument Panel, Gages and Console.