For 1990-2009 cars

### Removal Procedure

1. Door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the inside door handle housing rivets.
3. Remove the inside door handle housing.
4. Remove the control rods (2, 3, 4, 7) from the handle and lock. Refer to Door Linkage Replacement .
5. Remove the harness from the switches, if equipped.

### Installation Procedure

1. Install the harness to switches (if equipped).
2. Install the control rods (2, 3, 4, 7) to the handle and lock.
3. Install the inside door handle housing.
4. Install the inside door handle housing rivets.
5. Install the door trim panel. Refer to Door Trim Panel Replacement .