For 1990-2009 cars

Important: Replace the torque converter if it does not meet specifications.

1. Measure the OD of torque converter hub (1) at dimension A, the bushing wear area.

Torque Converter Hub OD
Dimension A must equal or exceed 58.250 mm (2.293 in).

2. Measure the distance between the flats of the torque converter hub at dimension A.

Torque Converter Hub Flats
Dimension A must equal or exceed 51.816 mm (2.040 in).

3. Measure the OD of the torque converter cover pilot at dimension A.

Torque Converter Pilot
Dimension A must equal or exceed 43.080 mm (1.696 in).