For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner . Refer to Air Cleaner Replacement .
2. Remove the accumulator bottle bracket retaining nuts and position the bottle out of the way.
3. Disconnect the wiring harness retainers.
4. Remove the MAXI fuse block and relay center retaining bolt and position out of the way.
5. Remove the 4 multi-use bracket nuts, reposition the control module bracket to the service position, and reinstall 2 of the fasteners.

### Installation Procedure

1. Reposition the multi-use module bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the multi-use module bracket nuts.

Tighten
Tighten the nuts to 25 N·m (18 lb ft).

3. Reposition the MAXI fuse block and relay center.

Tighten
Tighten the bolt to 9 N·m (80 lb in).

4. Reposition the wiring harness.
5. Install the wiring harness retainers.
6. Reposition the accumulator bottle in the accumulator bottle bracket.
7. Install the accumulator bottle bracket nuts.

Tighten
Tighten the nuts to 9 N·m (80 lb in).

8. Install the air cleaner . Refer to Air Cleaner Replacement .