For 1990-2009 cars

#### Tools Required

• | J 24420-C Harmonic Balancer Puller

• | J 42845 Crankshaft Balancer Installer

• | J 42847 Flywheel Holding Tool

### Removal Procedure

1. Remove the fan shroud. Refer to Fan Shroud Replacement in Engine Cooling.
2. Remove the drive belt. Refer to Drive Belt Replacement .
3. Remove the starter motor. Refer to Starter Motor Replacement in Engine Electrical.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: Make sure the teeth of the flywheel holding tool engage the engine flywheel teeth.

4. Install the J 42847 to the starter bolt holes.

Tighten
Tighten the J 42847 bolts to 50 N·m (37 lb ft).

5. Install the J 24420-C or equivalent onto the crankshaft balancer.
6. Tighten the center screw of the J 24420-C until the crankshaft balancer is clear of the crankshaft nose.
7. Remove the crankshaft balancer.
8. Clean and inspect the crankshaft balancer.

### Installation Procedure

Important:

• | The balancer should be positioned onto the end of the crankshaft as straight as possible prior to tool installation.

• | Apply grease or clean engine oil to the inside of the crankshaft balancer or the end of the crankshaft, to prevent galling during assembly.

1. Install the balancer onto the end of the crankshaft.
2. Install J 42845 to the crankshaft balancer.

Important: Apply the lubricant that comes with J 42845 each time the tool is used. Failure to lubricateJ 42845 may prevent the balancer from installing completely.

3. Using J 42845 install the balancer.
4. Tighten the J 42845 until the crankshaft balancer is completely seated against the crankshaft sprocket.
5. Remove the J 42845 from the crankshaft.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the crankshaft washer and bolt.

Tighten
Tighten the crankshaft balancer bolt to 225 N·m (189 lb ft).

7. Remove the J 42847 .
8. Install the starter motor. Refer to Starter Motor Replacement in Engine Electrical.
9. Install the drive belt. Refer to Drive Belt Replacement .
10. Install the fan shroud. Refer to Fan Shroud Replacement in Engine Cooling.