For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector from the relay.
2. Remove the following from the chassis:

• | The nut

• | The washer

• | The bolt

• | The axle shift motor relay

### Installation Procedure

1. Install the following to the chassis:

• | The axle shift motor relay

• | The bolt

• | The washer

• | The nut

2. Connect the electrical connector to the relay.