For 1990-2009 cars

### Removal Procedure

1. Remove the drum. Refer to Propeller Shaft Parking Brake Drum Replacement .
2. Remove the drum brake shoes and hardware. Refer to Parking Brake Shoe Replacement .
3. Remove the park brake hardware.

### Installation Procedure

Important: Prior to installation, apply a high temperature silicone lubricant to all brake component metal contact points. Examples include the point at which the brake shoe metal contacts the following parts:

• | The backing plate

• | The wheel cylinder

• | The adjustment strut

1. Replace the park brake hardware components as necessary.
2. Install the drum brake shoes and hardware. Refer to Parking Brake Shoe Replacement .
3. Install the drum. Refer to Propeller Shaft Parking Brake Drum Replacement .