For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Actuator Screws | 2 N·m | 18 lb in
Air Defroster Duct (Inboard) Screw | 1 N·m | 9 lb in
Air Defroster Duct (Outboard) Screw | 2 N·m | 18 lb in
Air Defroster Duct Screw | 2 N·m | 18 lb in
A-Pillar Ground Nut | 3 N·m | 27 lb in
Blower Motor Resistor Screw | 1 N·m | 9 lb in
Door Pillar Stud Nut | 3 N·m | 27 lb in
Floor Air Outlet Duct Screw | 1.9 N·m | 17 lb in
Heater Inlet/Outlet Hose Bracket Bolt | 6 N·m | 53 lb in
Heater Hose Clip Nut | 16 N·m | 12 lb in
Heater Inlet Fitting | 19 N·m | 14 lb in
HVAC Control Assembly Screw | 2 N·m | 18 lb in
HVAC Module Assembly Bolt | 11 N·m | 97 lb in
HVAC Module Assembly Nut | 3 N·m | 27 lb in
HVAC Module Upper Bolt | 7 N·m | 62 lb in
HVAC Control Module Assembly Screw | 2 N·m | 18 lb in
Instrument Panel Cluster Bezel Assembly Screw | 2 N·m | 18 lb in
IP Mounting Bracket Screw | 2 N·m | 18 lb in
Module Mounting Bolt | 11 N·m | 97 lb in
Module Mounting Nut | 2.8 N·m | 25 lb in
Module Mounting Screw | 1.9 N·m | 17 lb in
Right Lower IP Support Bolt | 2 N·m | 18 lb in
Vent Cable Clip Screw Right | 1 N·m | 9 lb in
Vent Cable Screw Left | 1 N·m | 9 lb in