For 1990-2009 cars

### Removal Procedure

1. Insert a small flat-bladed tool into the slot from the bottom. If equipped disconnect the electrical.
2. Press slightly in order to release it from the tab.
3. Slide the mirror off of the support.

### Installation Procedure

1. Install the mirror to the inside rearview mirror support. If equipped install the electrical connector.
2. Install the inside rearview mirror by sliding it downward firmly until it locks in place.