For 1990-2009 cars

Important:

• | Perform the following measurements at 3 or more locations.

• | Check the plates for coning on a level surface.

• | Replace any parts not meeting specifications.

1. Measure the thickness of each 2nd clutch fiber plate (1) at dimension A.

Specification
The 2nd clutch fiber plate minimum thickness is 2.375 mm (0.0935 in).

2. Measure the oil groove depth of each 2nd clutch fiber plate (1) at dimension B.

Specification
The 2nd clutch fiber plate oil groove minimum depth is 0.2 mm (0.0079 in).

3. Measure the cone of each 2nd clutch fiber plate (1) at dimension A.

Specification
The 2nd clutch fiber plate maximum cone is 0.225 mm (0.0089 in).

4. Measure the thickness of each 2nd clutch steel plate (1) at dimension A.

Specification
The 2nd clutch steel plate minimum thickness is 2.44 mm (0.096 in).

5. Measure the cone of each 2nd clutch steel plate (1) at dimension A.

Specification
The 2nd clutch steel plate maximum cone is 0.4 mm (0.0157 in).

6. Measure the thickness of the 2nd clutch spring plate (1) at dimension A.

Specification
The 2nd clutch spring plate minimum thickness is 3.11 mm (0.1224 in).

7. Measure the cone of the 2nd clutch spring plate (1) at dimension A.

Specification
The 2nd clutch spring plate maximum cone is 0.4 mm (0.0157 in).