For 1990-2009 cars

### Removal Procedure

1. Remove the brake hose from the chassis brake pipe.
2. Remove the retainer.
3. Remove the brake pipe.
4. Plug or cap the brake pipe.
5. Remove the bracket mounting bolts.
6. Remove the brake hose from the caliper.
7. Remove the brake hose mounting bracket.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the brake hose mounting bracket.

Tighten
Tighten the mounting bolts to 32 N·m (24 lb ft).

2. Install the brake pipes.

Tighten
Tighten the brake pipe fittings to 19 N·m (14 lb ft).

3. Install the brake hose through the frame bracket.
4. Connect the fitting to the brake hose.

Tighten
Tighten the fitting to 19 N·m (14 lb ft).

5. Install the retainer.
6. Bleed the brakes. Refer to Hydraulic Brake System Bleeding .