For 1990-2009 cars

Icon | Icon Definition
--- | ---
| Important: The LG5 charging system circuit has a resistance wire for circuit 25 (WHT). The wire provides a resistive current flow to the generator. The resistance wire will allow the generator to operate properly even if the charge indicator circuit fails or the charge indicator bulb burns out.

• | The wire length is 48.1 cm (19 in).

• | The wire size is 0.22 mm²--AWG Size 24 gage.

• | The wire provides a resistance of 20 ohms (±2 ohms).

Be sure to maintain 20 ohms (±2 ohms) circuit resistance when repairing this circuit.