For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Spring Frame Hanger to Frame Locknut | 330 N·m | 243 lb ft
Air Spring to Air Spring Frame Hanger Locknut | 34 N·m | 25 lb ft
Air Suspension Relief Valve Bolt | 18 N·m | 13 lb ft
Cross Channel to Main Support Beam Locknut | 330 N·m | 243 lb ft
Leveling Valve Arm on Leveling Valve Locknut | 23 N·m | 17 lb ft
Leveling Valve Mounting Locknut - Except GPG | 95 N·m | 70 lb ft
Leveling Valve Mounting Locknut - With GPG | 82 N·m | 61 lb ft
Rebound Bolt Locknut | 82 N·m | 61 lb ft
Shock Absorber to Mounting Bracket Locknut | 85 N·m | 63 lb ft
Transverse Rod Bar Pin Nut - Except GPG | 298 N·m | 220 lb ft
Transverse Rod Taper Pin Locknut - With GPG | 508 N·m | 375 lb ft
Torque Bar Rod Pin Locknut | 241 N·m | 178 lb ft
Torque Rod Locknut | 241 N·m | 178 lb ft
Torque Rod Locknut at Axle End of Torque Rod | 241 N·m | 178 lb ft
U-bolt Nuts | 394 N·m | 291 lb ft
10 mm (0.375 in) Hex Head Self-Tapping Screw | 34 N·m | 25 lb ft