For 1990-2009 cars

### Removal Procedure

1. Tilt the hood open.
2. Remove the clip retaining the wheel housing panel to the radiator support bracket.
3. Remove the wheel housing panel, from the retainer tabs.
4. Remove the wheel house panel from the vehicle.

### Installation Procedure

1. Install the wheel housing panel to the retainer tabs.
2. Install the clip retaining the front of the panel to the radiator support bracket.
3. Close the hood.