For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle, if required. Refer to Lifting and Jacking the Vehicle in General Information.
2. If equipped with the 1.75 inch or 1.5 inch pilot shaft spline, remove the clutch fork return spring.
3. If equipped with the 8.1L engine, and regular production options (RPOs) MM7/MNC/MPU/MSC/MSG, and the 13 inch clutch, remove the clutch cable retainer nuts (2).
4. Remove the clutch cable swivel (1) from the cable.
5. Remove the clutch cable retainer (3).
6. Remove the clutch cable from the clutch fork.
7. Remove the clutch fork boot bolts.
8. Remove the clutch fork retainer and boot.
9. Remove the flywheel housing cover bolts and cover.
10. Using a pry bar, remove the clutch fork from the flywheel housing ball stud.
11. Remove the clutch fork.

### Installation Procedure

1. Install the clutch fork.
2. Lubricate the ball stud using GM P/N 12378484 or equivalent.
3. Install the clutch fork over the release bearing.
4. Install the clutch fork to the flywheel housing ball stud.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the flywheel housing cover and bolts.

Tighten
Tighten the flywheel housing cover bolts to 12 N·m (106 lb in).

6. Install the clutch fork retainer and boot.
7. Install the clutch fork boot bolts.
8. Route the clutch cable through the clutch fork.
9. Install the clutch cable retainer (3).
10. If equipped with the 8.1L engine, and RPOs MM7/MNC/MPU/MSC/MSG, and the 13 inch clutch, install the clutch cable swivel (1) to the cable.
11. Install the clutch cable retainer nuts (2).
12. If equipped with the 1.75 inch or 1.5 inch pilot shaft spline, install the clutch fork return spring.
13. Adjust the clutch cable. Refer to Clutch Pedal Free Travel Adjustment .
14. Lower the vehicle, if required.