For 1990-2009 cars

### Removal Procedure

1. Remove the hydraulic lines or the air lines from the radiator shutter control valve. Refer to Shutter Control Valve Hose Replacement .
2. Remove the electrical connector to the radiator shutter control valve.
3. Remove the fittings from the control valve.
4. Remove the radiator shutter control valve mounting nut.
5. Remove the radiator shutter control valve from the radiator lower mounting panel.

### Installation Procedure

1. Install the radiator shutter control valve to the radiator lower mounting panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the radiator shutter control valve mounting nut.

Tighten
Tighten the radiator shutter control valve mounting nut to 13 N·m (115 lb in).

3. Install the electrical connector to the radiator shutter control valve.
4. Install the fittings to the control valve.

Tighten

• | Tighten the air fitting to 6 N·m (53 lb in).

• | Tighten the hydraulic fitting to 20 N·m (15 lb ft).

5. Install the hydraulic lines or the air lines, as equipped, to the radiator shutter control valve.