For 1990-2009 cars

#### Tools Required

J 9886-01 Regulator Handle Tool

### Removal Procedure

1. Insert the J 9886-01 (3) between the handle (1) and the bearing plate.
2. Align the tool parallel with the door handle, and push in order to disengage the clip (2).
3. Remove the window regulator handle.
4. Pull the handle from the door.
5. Remove the bearing plate.

### Installation Procedure

1. Install the bearing plate to the trim panel.
2. Install the window regulator handle.
3. Raise the window.
4. Push the clip onto the handle.
5. Insert the handle onto the regulator shaft so the handle is horizontal and the knob points toward the front of the door.
6. Push the handle until the clip engages the window regulator shaft.