For 1990-2009 cars

## Front Disc Brake Pads Replacement Bendix

### Removal Procedure

Notice: Support the brake caliper with heavy mechanic wire, or equivalent, whenever it is separated from its mount and the hydraulic flexible brake hose is still connected. Failure to support the caliper in this manner will cause the flexible brake hose to bear the weight of the caliper, which may cause damage to the brake hose and in turn may cause a brake fluid leak.

1. Remove the brake caliper (5). Refer to Front Brake Caliper Replacement .

Do not remove the brake line from the caliper.

2. Remove the inner brake pad from the brake caliper mounting plate (4).
3. Slide the outer brake pad along the rail in the brake caliper housing to the notches.
4. Remove the outer brake pad.

### Installation Procedure

1. Inspect the brake caliper. Refer to Brake Caliper Inspection .
2. Install the outer brake pad into the brake caliper housing.
3. Install the inner brake pad onto the brake caliper mounting plate.
4. Install the brake caliper (5). Refer to Front Brake Caliper Replacement .

## Front Disc Brake Pads Replacement Dayton-Welther

### Removal Procedure

Notice: Refer to Brake Caliper Notice in the Preface section.

1. Remove the brake caliper (5). Refer to Front Brake Caliper Replacement .

Do not remove the brake line from the caliper.

2. Remove the brake pad retainer spring.
3. Slide the outer brake pad along the rail in the brake caliper housing to the notches.
4. Remove the outer brake pad.
5. Slide the inner brake pad along the rail in the brake caliper housing to the notches.
6. Remove the inner brake pad.

### Installation Procedure

1. Inspect the brake caliper. Refer to Brake Caliper Inspection .
2. Install the inner brake pad.
3. Install the outer brake pad.
4. Install a new brake pad retainer spring.
5. If the service kit includes extra springs, discard the springs.
6. Install the brake caliper (5). Refer to Front Brake Caliper Replacement .