For 1990-2009 cars

### Circuit Description

An ignition voltage is supplied directly to the evaporative emission (EVAP) canister purge solenoid valve. The EVAP purge solenoid valve is pulse width modulated (PWM). The control module controls the EVAP purge solenoid valve ON time by grounding the control circuit via an internal switch called a driver. The scan tool displays the amount of ON time as a percentage. The control module monitors the status of the driver. If the control module detects an incorrect voltage for the commanded state of the driver, DTC P0443 sets.

### Conditions for Running the DTC

• | The engine speed is more than 400 RPM.

• | The system voltage is between 6-18 volts.

### Conditions for Setting the DTC

• | The control module detects that the commanded state of the driver and the actual state of the control circuit do not match.

• | The above conditions are present for a minimum of 5 seconds.

### Action Taken When the DTC Sets

• | The control module illuminates the malfunction indicator lamp (MIL) on the second consecutive ignition cycle that the diagnostic runs and fails.

• | The control module records the operating conditions at the time the diagnostic fails. The first time the diagnostic fails, the control module stores this information in the Failure Records. If the diagnostic reports a failure on the second consecutive ignition cycle, the control module records the operating conditions at the time of the failure. The control module writes the operating conditions to the Freeze Frame and updates the Failure Records.

### Conditions for Clearing the MIL/DTC

• | The control module turns OFF the malfunction indicator lamp (MIL) after 3 consecutive ignition cycles that the diagnostic runs and does not fail.

• | A current DTC, Last Test Failed, clears when the diagnostic runs and passes.

• | A history DTC clears after 40 consecutive warm-up cycles, if no failures are reported by this or any other emission related diagnostic.

• | Clear the MIL and the DTC with a scan tool.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step tests if the concern is active. An audible clicking sound should be heard or felt when the EVAP canister purge solenoid valve is commanded to 50 percent and should stop when the EVAP canister purge solenoid valve is commanded to 0 percent. The rate at which the valve cycles should increase as the commanded state is increased and decrease as the commanded state is decreased. Repeat the commands as necessary.

2. This step verifies that the control module is providing ground to the EVAP canister purge solenoid valve.

3. This step tests if a ground is constantly being applied to the EVAP canister purge solenoid valve.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Engine Controls Schematics Connector End View Reference: Powertrain Control Module Connector End Views or Engine Controls Connector End Views
1 | Did you perform the Diagnostic System Check - Engine Controls? | Go to Step 2 | Go to Diagnostic System Check - Engine Controls
2 |

1. Turn ON the ignition, with the engine OFF.
2. Command the evaporative emission (EVAP) canister purge solenoid valve to 50 percent and then to 0 percent with a scan tool.

Do you hear or feel a clicking from the EVAP canister purge solenoid valve when the scan tool is commanded to 50 percent?

Go to Step 3

Go to Step 4

3 |

1. Observe the Freeze Frame/Failure Records for this DTC.
2. Turn OFF the ignition for 30 seconds.
3. Start the engine.
4. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text or as close to the Freeze Frame/Failure Records data that you observed.

Does the DTC fail this ignition?

Go to Step 4

Go to Intermittent Conditions

4 |

1. Turn OFF the ignition.
2. Disconnect the EVAP canister purge solenoid valve harness connector.
3. Turn ON the ignition, with the engine OFF.
4. Probe the ignition voltage circuit at the EVAP canister purge solenoid valve harness connector with a test lamp connected to a good ground.

Does the test lamp illuminate?

Go to Step 5

Go to Step 11

5 |

1. Connect a test lamp between the control circuit and the ignition voltage circuit of the EVAP purge solenoid valve harness connector.
2. Command the EVAP canister purge solenoid valve to 0 percent with a scan tool.

Does the test lamp illuminate?

Go to Step 8

Go to Step 6

6 | Command the EVAP canister purge solenoid valve to 50 percent with a scan tool. Does the test lamp illuminate or pulse when the EVAP canister purge solenoid valve is commanded to 50 percent? | Go to Step 9 | Go to Step 7
7 | Test the control circuit of the EVAP canister purge solenoid valve for an open or short to voltage. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 14 | Go to Step 10
8 | Test the control circuit of the EVAP canister purge solenoid valve for a short to ground. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 14 | Go to Step 13
9 | Inspect for poor connections at the harness connector of the EVAP canister purge solenoid valve. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 14 | Go to Step 12
10 | Inspect for poor connections at the harness connector of the powertrain control module (PCM). Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 14 | Go to Step 13
11 | Repair the ignition voltage circuit of the EVAP purge solenoid valve for an open or a short to ground. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | Go to Step 14 | --
12 | Replace the EVAP canister purge solenoid valve. Did you complete the replacement? | Go to Step 14 | --
13 | Replace the control module. Refer to Powertrain Control Module Replacement . Did you complete the replacement? | Go to Step 14 | --
14 |

1. Clear the DTCs with a scan tool.
2. Turn OFF the ignition for 30 seconds.
3. Start the engine.
4. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text.

Does the DTC run and pass?

Go to Step 15

Go to Step 2

15 | With a scan tool, observe the stored information, Capture Info. Does the scan tool display any DTCs that you have not diagnosed? | Go to Diagnostic Trouble Code (DTC) List | System OK