For 1990-2009 cars

Table 1: | Fuel Injector Balance Test Example (Typical)

(1) | First Fuel Pressure Gage Reading
(2) | Second Fuel Pressure Gage Reading

#### Fuel Injector Balance Test Example (Typical)

Cylinder | 1 | 2 | 3 | 4
--- | --- | --- | --- | ---
1st Reading | 296 kPa (43 psi) | 296 kPa (43 psi) | 296 kPa (43 psi) | 296 kPa (43 psi)
2nd Reading | 131 kPa (19 psi) | 117 kPa (17 psi) | 124 kPa (18 psi) | 145 kPa (21 psi)
Amount of Drop | 165 kPa (24 psi) | 179 kPa (26 psi) | 172 kPa (25 psi) | 151 kPa (22 psi)
Average Range: 156-176 kPa (22.5-25.5 psi) | Injector OK | Replace fuel injector - too much fuel pressure drop | Injector OK | Replace fuel injector - too little fuel pressure drop

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. The engine coolant temperature must be below the operating temperature in order to avoid irregular fuel pressure readings due to hot soak fuel boiling.

2. If the pressure drop value for each fuel injector is within 10 kPa (1.5 psi) of the average pressure drop value, the fuel injectors are flowing properly. Calculate the pressure drop value for each fuel injector by subtracting the second pressure reading from the first pressure reading. Refer to the illustration above.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check-Engine Controls? | -- | Go to Step 2 | Go to Diagnostic System Check - Engine Controls
2 | Did you perform the Fuel Injector Coil Test? | -- | Go to Step 3 | Go to Fuel Injector Solenoid Coil Test
3 | Important : Do not perform this test if the engine coolant temperature is above 94°C (201°F). Observe the ECT parameter with a scan tool. Does the scan tool indicate that the ECT parameter is less than the specified value? | 94°C (201°F) | Go to Step 4 | --
4 | Important: Verify there is adequate fuel in the fuel tank before proceeding with this diagnostic.

1. Turn OFF the ignition.
2. Install the fuel pressure gage. Refer to Fuel Pressure Gage Installation and Removal .
3. Turn ON the ignition, with the engine OFF.
4. Command the fuel pump ON with a scan tool.

Important:

• | It may be necessary to command the fuel pump ON a few times, in order to obtain the highest possible fuel pressure.

• | Do not start the engine.

5. Observe the fuel pressure gage, with the fuel pump commanded ON.

Is the fuel pressure within the specified range?

384-425 kPa (55-62 psi)

Go to Step 5

Go to Fuel System Diagnosis

5 | Important: The fuel pressure may vary slightly when the fuel pump stops operating. After the fuel pump stops operating, the fuel pressure should stabilize and remain constant. Monitor the fuel pressure gage for 1 minute. Does the fuel pressure drop more than the specified value? | 34 kPa (5 psi) | Go to Fuel System Diagnosis | Go to Step 6
6 |

1. Connect the J 39021 Fuel Injector Tester and the J 39021-380 Fuel Injector Test Harness to a fuel injector.
2. Set the amperage supply selector switch on the fuel injector tester to the Balance Test 0.5-2.5 amp position.
3. Command the fuel pump ON and then OFF with a scan tool.
4. Record the fuel pressure indicated by the fuel pressure gage after the fuel pressure stabilizes. This is the first pressure reading.

Important: Record the fuel pressure value immediately after the fuel injector stops pulsing. The fuel pressure may rise after the fuel injector stops pulsing. Do not record the higher fuel pressure value.

5. Energize the fuel injector by depressing the Push to Start Test button on the fuel injector tester.
6. Record the fuel pressure indicated by the fuel pressure gage. This is the second fuel pressure reading.
7. Repeat steps 1 through 6 for each fuel injector.
8. Subtract the second pressure reading from the first pressure reading for one fuel injector. The result is the pressure drop value.
9. Obtain a pressure drop value for each fuel injector.
10. Add all of the individual pressure drop values. This is the total pressure drop.
11. Divide the total pressure drop by the number of fuel injectors. This is the average pressure drop.

Does any fuel injector have a pressure drop value that is more than the average pressure drop or less than the average pressure drop by the specified value?

10 kPa (1.5 psi)

Go to Step 7

Go to Symptoms - Engine Controls

7 | Perform the Fuel Injector Cleaning . Did you complete the procedure? | -- | Go to Step 8 | --
8 | Operate the vehicle in order to verify the repair. Does a driveability condition still exist? | -- | Go to Symptoms - Engine Controls | System OK