For 1990-2009 cars

### Removal Procedure

1. Locate the door jamb switch.

The switch is under the left side of the instrument panel.

2. Squeeze together the tangs of the switch.
3. Push the switch through the side of the instrument panel.
4. Disconnect the door jamb switch electrical connector of the door jamb switch.
5. Remove the door jamb switch from the vehicle.

### Installation Procedure

1. Connect the electrical connector of the door jamb switch.
2. Squeeze together the tangs of the switch.
3. Push the switch through the side of the instrument panel.