For 1990-2009 cars

#### Tools Required

• | J 43767 Tone Wheel Staker

• | J 43768 Tone Wheel Driver

#### Removal Procedure

1. Grind the stakes from the 1-2-3-4, 4-5 clutch housing (1).
2. Position the 1-2-3-4, 4-5 clutch housing (2) on a press so that the front of the housing is down.
3. Install J 43768 (1) onto the tone wheel (3).
4. Using J 43768 (1), press the tone wheel (3) from the 1-2-3-4, 4-5 clutch housing (2).

### Installation Procedure

1. Position the 1-2-3-4, 4-5 clutch housing (3) on a press so that the front of the housing is facing up.
2. Align the tone wheel (2) so that the outside edge is facing up.
3. Install the tone wheel (2) onto the 1-2-3-4, 4-5 clutch housing.
4. Install J 43768 (1) onto the tone wheel.
5. Using J 43768 (1), press the tone wheel onto the 1-2-3-4, 4-5 clutch housing.
6. Locate 4 positions on the 1-2-3-4, 4-5 clutch housing (3), 90 degrees apart from each other, that have not been previously staked .
7. Install J 43767 onto the 1-2-3-4, 4-5 clutch housing with the 2 staking prongs at 2 of the 4 staking positions.
8. Install J 43768 (1) onto J 43767 (2).

Notice: Stake the tone wheel to 9 tons. The accuracy of the pressure gauges on presses varies. Start at a lower pressure and increase to 9 tons. Too great a pressure will distort the tone wheel. Too little pressure will result in stakes that will not hold.

9. Stake the tone wheel to the 1-2-3-4, 4-5 clutch housing.

Important: If necessary, tap J 43768 and J 43767 to remove the tools from the 1-2-3-4, 4-5 clutch housing.

10. Remove the J tools and repeat steps 7-9 at the remaining 2 staking positions.
11. Remove the J tools.