For 1990-2009 cars

### Removal Procedure

Notice: Do not start the vehicle with any power steering gear inlet or outlet hoses disconnected. When disconnected, plug or cap all openings of components. Failure to do so could result in contamination or loss of power steering fluid and damage to the system.

1. Install a drain pan under the vehicle.
2. Siphon the fluid from the reservoir to prevent excessive spillage.
3. Remove the reservoir inlet hose (3) from the Power Steering Gear.
4. Remove the reservoir inlet hose from the reservoir.
5. Remove the hose from the vehicle.

### Installation Procedure

Notice: The inlet and outlet hoses must not be twisted during installation. Do not bend or distort the inlet or outlet hoses to make installation easier. Failure to follow these procedures could result in component damage.

1. Route the hose in the same position the hose occupied prior to removal.
2. Smoothly route the hose in order to avoid sharp bends and kinking.
3. Install the reservoir inlet hose to the reservoir.

Position the clamp at the end of the hose.

4. Fully crimp the clamp to the hose.
5. Install the reservoir inlet hose to the Power Steering Gear.
6. Check the power steering fluid level. Refer to Checking and Adding Power Steering Fluid .
7. Remove the drain pan from under the vehicle.
8. Bleed the power steering system. Refer to Power Steering System Bleeding .