For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Seat Belt Schematics
1 |

1. Turn OFF the ignition.
2. Disconnect the seat belt alarm.
3. Turn ON the ignition, with the engine OFF.

Does the fasten safety belt indicator turn OFF?

Go to Step 4

Go to Step 2

2 | Test the fasten safety belt indicator control circuit between the seat belt alarm and the driver information center - right for a short to voltage. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 5 | Go to Step 3
3 | Replace the DIC - right. Did you complete the repair? | Go to Step 5 | --
4 | Replace the seat belt alarm. Did you complete the replacement? | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 1