For 1990-2009 cars

### Removal Procedure

Important: When replacing battery cables, use a replacement cable that is the same type, diameter, and length. Additional feed wires may be attached to the positive cables. Additional ground leads may be attached to the negative cables. Always route a replacement battery cable the same as the original cable routing.

1. Follow the above precautions when servicing the battery and cables.
2. Remove the battery carrier cover.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

3. Remove the negative battery cable.
4. Remove the positive cable from the starter solenoid.
5. Remove the positive cable from the battery.
6. Remove the positive cable clamps and tie downs.
7. Remove the positive cable from the vehicle.

### Installation Procedure

1. Connect the negative cable to the engine.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Connect the negative cable to the frame.

Clean the grounding area and coat it with a copper-impregnated ground sealer.

Tighten

• | Tighten the cable to the engine bolt to 30 N·m (22 lb ft).

• | Tighten the cable to the frame rail nut to 30 N·m (22 lb ft).