For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Pitman Arm to Gear Clamp Nut-Family 2 | 325 N·m | 240 lb ft
Pitman Arm to Gear Nut-Family 3 | 370 N·m | 275 lb ft
Relay Rod to Pitman Arm Nut-FN9/FM7 | 210 N·m | 155 lb ft
Relay Rod to Pitman Arm Nut-FM8 | 129 N·m | 96 lb ft
Relay Rod to Pitman Arm Nut-FM6/FS7/FL3/FH4 | 162 N·m | 120 lb ft
Relay Rod to Steering Arm Nut-FN9/FM7/FM8 | 210 N·m | 155 lb ft
Relay Rod to Steering Arm Nut-FM6/FS7/FL3/FH4 | 325 N·m | 239 lb ft
Steering Arm-to-Knuckle Bolt --16K Axle | 567 N·m | 820 lb ft
Tie Rod Arm to Knuckle Bolt-16K Axle | 567 N·m | 420 lb ft
Tie Rod Ball Joint to Steering Arm Nut-FN9/FM7/FM8 | 210 N·m | 155 lb ft
Tie Rod Ball Joint to Steering Arm Nut -FM6/FS7/FL3/FH4 | 325 N·m | 239 lb ft
Tie Rod Tube Clamp Bolt Nut | 75 N·m | 55 lb ft