For 1990-2009 cars

Caution: The 1000 Series™ transmission dry weight is approximately 150 kg (330 lb). To help avoid personal injury and/or property damage: Use caution when installing, removing, or moving the transmission. Get help when lifting the transmission. Assistance from a hoist or another person may be required. Ensure that lifting equipment can properly support the transmission.

1. Attach a sling to the transmission.
2. Attach a hoist to the sling.
3. Put moderate lift tension on the hoist.
4. Disconnect and remove the transmission from the repair stand.
5. Place the transmission on the work table with the oil pan facing down.
6. Install the power take-off (PTO) cover gaskets (1)
7. Install 2 PTO covers (2).

Notice: Refer to Fastener Notice in the Preface section.

8. Install 12 PTO cover bolts (3).

Tighten
Tighten the bolts to 43 N·m (31 lb ft).