For 1990-2009 cars

## Engine Flywheel Installation Automatic Transmission

Important: Ensure the flex plate is installed correctly. Engine Side is stamped on the flex plate to assist with installation.

1. Install the flex plate.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts.

Tighten the bolts following a criss-cross pattern.

Tighten

1. Tighten the bolts a first pass in sequence to 40 N·m (30 lb ft).
2. Tighten the bolts a second pass in sequence to 80 N·m (59 lb ft).
3. Tighten the bolts a final pass in sequence to 100 N·m (74 lb ft).

## Engine Flywheel Installation Manual Transmission

1. Install the engine flywheel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the engine flywheel bolts.

Tighten the fasteners following a criss-cross pattern.

Tighten

1. Tighten the bolts a first pass in sequence to 40 N·m (30 lb ft).
2. Tighten the bolts a second pass in sequence to 80 N·m (59 lb ft).
3. Tighten the bolts a final pass in sequence to 100 N·m (74 lb ft).