For 1990-2009 cars

### Circuit Description

The powertrain control module (PCM) uses the throttle position (TP), barometric pressure (BARO), intake air temperature (IAT), and engine RPM in order to calculate an expected mass air flow (MAF) rate. The PCM compares this value to the MAF value and the speed density calculation in order to verify the proper throttle operation.

### Conditions for Running the DTC

• | DTCs P0601, P0602, P0604, P0606, P1515, P1516, P1517, or P1518 are not set.

• | DTCs P1120, P1220 and P1221 are not set at the same time or DTC P1120 and P1220 are not set at the same time.

• | The engine operates longer than 1 second.

• | The engine speed is greater than 500 RPM.

### Conditions for Setting the DTC

• | The PCM detects that the difference between the actual airflow (MAF) and the speed density calculated airflow is greater than expected.

• | All of the above conditions are met for less than 1 second.

### Action Taken When the DTC Sets

• | The control module illuminates the malfunction indicator lamp (MIL) when the diagnostic runs and fails.

• | The control module records the operating conditions at the time the diagnostic fails. The control module stores this information in the Freeze Frame and/or the Failure Records.

• | The control module commands the TAC system to operate in the Reduced Engine Power mode.

• | A message center or an indicator displays Reduced Engine Power.

• | Under certain conditions the control module commands the engine OFF.

### Conditions for Clearing the MIL/DTC

• | The control module turns OFF the malfunction indicator lamp (MIL) after 3 consecutive ignition cycles that the diagnostic runs and does not fail.

• | A current DTC, Last Test Failed, clears when the diagnostic runs and passes.

• | A history DTC clears after 40 consecutive warm-up cycles, if no failures are reported by this or any other emission related diagnostic.

• | Clear the MIL and the DTC with a scan tool.

### Diagnostic Aids

• | Inspect the throttle blade for being broken, bent, or missing.

• | Inspect the TP sensor for proper installation. A sensor that is mis-aligned could set this DTC.

• | Inspect the throttle actuator control (TAC) module connectors for signs of water intrusion. When this occurs, multiple DTCs could be set with no circuit or component conditions found during diagnostic testing.

• | Physically/visually inspect the throttle body assembly and correct any problems that you observe. Manually move the throttle blade from closed to wide open throttle (WOT). You should not need to use excessive force. The throttle blade should move smoothly through the full range and should return to a slightly open position on its own.

• | When the TAC module detects a condition within the TAC system, more than one TAC system related DTC may set. This is due to the many redundant tests run continuously on this system. Locating and repairing one individual condition may correct more than one DTC. Disconnecting components during testing may set additional DTCs. Keep this in mind when reviewing the stored information, Capture Info.

• | For an intermittent condition, refer to Intermittent Conditions .

### Test Description

The number below refers to the step number on the diagnostic table.

1. When the TAC module detects a condition within the TAC system, more than one TAC system related DTC may set. This is due to the many redundant tests run continuously on this system. Locating and repairing one individual condition may correct more than one DTC. Disconnecting components during testing may set additional DTCs. Keep this in mind when reviewing the stored information, Capture Info.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Engine Controls Schematics
1 | Did you perform the Diagnostic System Check-Engine Controls? | Go to Step 2 | Go to Diagnostic System Check - Engine Controls
2 | Is DTC P0102, P0103, P0107, P0108, P0112, P0113, P1111, or P1112 set? | Go to Diagnostic Trouble Code (DTC) List | Go to Step 3
3 | Important: If any of the conditions listed below exist, replace the throttle body assembly. Refer to Throttle Body Assembly Replacement . Inspect the throttle body for the following conditions:

• | TP sensor loose or damaged

• | Loose or damaged throttle blade

• | Cracked or bent throttle shaft

• | Drive mechanism damage

Did you find and correct the condition?

Go to Step 4

Go to Diagnostic Aids

4 |

1. Use the scan tool in order to clear the DTCs.
2. Turn OFF the ignition for 30 seconds.
3. Start the engine.
4. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text.

Does the DTC run and pass?

Go to Step 5

Go to Step 2

5 | With a scan tool, observe the stored information, Capture Info. Does the scan tool display any DTCs that you have not diagnosed? | Go to Diagnostic Trouble Code (DTC) List | System OK