For 1990-2009 cars

### Removal Procedure

1. Remove the radiator shutter assembly mounting bolts.
2. Remove the radiator shutter assembly from the radiator lower mounting panel.

### Installation Procedure

1. Install the radiator shutter assembly to the radiator lower mounting panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the radiator shutter assembly mounting bolts.

Tighten

• | Tighten the air radiator shutter mounting air bolt to 30 N·m (22 lb ft).

• | Tighten the hydraulic radiator shutter mounting hydraulic bolt to 40 N·m (30 lb ft).

3. Install the hydraulic lines or the air lines to the radiator shutter actuator.