For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Suspension Seat Bolt | 55 N·m | 41 lb ft
Bucket Seat Bolt | 55 N·m | 41 lb ft
High Back Seat Belt (Buckle Side) Bolt | 90 N·m | 66 lb ft
High Back Seat Belt Bracket Bolt | 90 N·m | 66 lb ft
Low Back Seat Belt (Buckle Side) Bolt | 40 N·m | 30 lb ft
Low Back Seat Belt Bracket Bolt | 40 N·m | 30 lb ft
Seat Belt (Buckle Side) or Unit Bolt | 55 N·m | 41 lb ft
Suspension Seat Bolt | 55 N·m | 41 lb ft
Three-Passenger Seat Bolt | 55 N·m | 41 lb ft
Two-Passenger Seat Bolt | 55 N·m | 41 lb ft