For 1990-2009 cars

## Turn Signal Cancel Cam and Steering Shaft Upper Bearing Spring Replacement On Vehicle

#### Tools Required

• | J 1859-A Steering Wheel Puller

• | J 23653-SIR Lock Plate Compressor

### Removal Procedure

1. Position the front wheels straight ahead.
2. Place the ignition switch in the LOCK position and remove the key.
3. Remove the horn pad assembly. Refer to Steering Wheel Horn Switch Replacement .
4. Remove the nut retainer clip (9) from the steering shaft.
5. Mark the steering wheel shaft (5) and the steering wheel (1) in order to allow installation in the same position as when removed.
6. Remove the steering wheel using J 1859-A . Refer to Steering Wheel Replacement .
7. Remove and dispose the bearing retainer (1) using the J 23653-SIR .
8. Remove the steering shaft spacer (1).
9. Remove the turn signal cancel cam (2).
10. Remove the upper bearing spring (3).

### Installation Procedure

1. Install the upper bearing spring (3).
2. Lubricate and install the turn signal cancel cam (2).
3. Install the steering shaft spacer (1).
4. Install the new bearing retainer using J 23653-SIR .
5. Align the marks which were made during the removal procedure and Install the steering wheel (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the steering wheel shaft nut (4).

Tighten
Tighten the steering wheel shaft nut to 40 N·m (30 lb ft).

7. Install the nut retainer clip (9) onto the steering shaft.
8. Install the horn pad assembly (3). Refer to Steering Wheel Horn Switch Replacement .