For 1990-2009 cars

### Removal Procedure

1. Open the driver door.
2. In order to remove the flasher module (1) from the instrument panel (IP) convenience center, simultaneously perform the following:

2.1. | Lift upward on the tab that retains the flasher module to the IP convenience center.

2.2. | Remove the flasher module from the IP convenience center.

### Installation Procedure

1. Position the flasher module (1) to the IP convenience center.
2. Engage the flasher module until fully seated and the retaining tab clicks.
3. Close the driver door.