For 1990-2009 cars

#### Tools Required

J 42849 Crankshaft Rear Seal Installer

Important: Crankshaft rear oil seal and engine flywheel installation requires adequate space for installation. If the engine stand does not allow suitable space to use the J 42849 , install the crankshaft rear oil seal and engine flywheel with the engine properly supported on the floor.

1. Make sure the crankshaft rear chamfer is free of grit, loose rust, and burrs. Correct as needed.
2. Apply a very light film of oil onto the crankshaft sealing surface.

DO NOT apply oil to the sealing surface of the engine block.

3. Install the seal on the J 42849 .
4. Position J 42849 against the crankshaft. Thread the attaching screws into the tapped holes in the crankshaft.
5. Tighten the screws securely with a screwdriver in order to ensure that the seal is installed squarely over the crankshaft.
6. Rotate the center nut until the J 42849 bottoms.
7. Remove the J 42849 .