For 1990-2009 cars

Use precision instruments in order to check the king pin inclination. King pin inclination is the difference of the measurements at points (1) and (2). If the axle is bent or twisted, refer to Front Axle Replacement . Straightening the axle center in order to correct the king pin inclination is not recommended and will also change the camber. Recheck the camber after correcting the king pin inclination.