For 1990-2009 cars

## Propeller Shaft Parking Brake Drum Replacement Bendix 229 mm (9 in)

### Removal Procedure

1. Block the wheels.
2. Remove the propeller shaft. Refer to the following list for the correct replacement procedure in Propeller Shaft:

• | One-Piece Propeller Shaft Replacement

• | Two-Piece Propeller Shaft Replacement

• | Three-Piece Propeller Shaft Replacement

• | Four-Piece Propeller Shaft Replacement

3. Remove the following components from the center of the yoke:

• | The companion flange bolt

• | The washer

• | The retainer

4. Straighten the lock tab on the washer.
5. Remove the brake drum (6) and the yoke assembly from the transmission.
6. Remove the bolts that hold the drum (6) to the yoke.

Important: Closely examine all mounting bolt holes in the drum for stress cracks.

7. Inspect the drum (6) for the following conditions:

• | Cracks

• | Scoring

• | Pitting

• | Grooves

• | Overheating damage

8. Repair the drum as needed.
9. Inspect the linings (1) for contamination and excessive wear. The minimum lining thickness, with bonded linings, is 1.52 mm (0.060 in).

If replacement is necessary, replace the linings as a set.

10. Inspect the brake mechanism for proper operation.

Repair the brake mechanism as needed.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the companion flange bolt and a new washer to the transmission mainshaft at the center of the yoke.

Tighten
Tighten the bolt to 140 N·m (103 lb ft).

2. Install the bolts that hold the drum (6) to the yoke.
3. Install the drum and yoke assembly to the transmission.
4. Install the propeller shaft. Refer to the following list for the correct replacement procedure in Propeller Shaft:

• | One-Piece Propeller Shaft Replacement

• | Two-Piece Propeller Shaft Replacement

• | Three-Piece Propeller Shaft Replacement

• | Four-Piece Propeller Shaft Replacement

5. Adjust the parking brake. Refer to Park Brake Adjustment .
6. Remove the wheel blocks.

## Propeller Shaft Parking Brake Drum Replacement Bendix 305 mm (12 in)

### Removal Procedure

1. Block the wheels.
2. Release the parking brake.
3. Raise up at least one rear wheel.
4. Remove the propeller shaft. Refer to the following list for the correct replacement procedure in Propeller Shaft:

• | One-Piece Propeller Shaft Replacement

• | Two-Piece Propeller Shaft Replacement

• | Three-Piece Propeller Shaft Replacement

• | Four-Piece Propeller Shaft Replacement

5. Remove the nuts that hold the yoke and the brake drum.
6. Remove the yoke.
7. Remove the drum. You may need to back the linings (17,25) off by turning the adjusting screw (21).

Important: Closely examine all of the mounting bolt holes in the drum for stress cracks.

8. Inspect the drum for the following conditions:

• | Cracks

• | Scoring

• | Pitting

• | Grooves

• | Overheating damage

9. Replace the drum as necessary.
10. Inspect the linings (17,25) for contamination and excessive wear. The minimum lining thickness with bonded linings is 1.52 mm (0.060 in).
11. If necessary, replace the linings (17,25) as a set.
12. Inspect the brake mechanism for proper operations.

Repair or replace the brake mechanism as necessary.

### Installation Procedure

1. Install the drum.
2. Install a new set of linings (17,25), if necessary. Use adjusting screw (21) to align linings to drum.
3. Install the yoke.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the nuts that hold the yoke and the brake drum.

Tighten
Tighten the nuts to 37 N·m (27 lb ft).

5. Install the propeller shaft. Refer to the following list for the correct replacement procedure in Propeller Shaft:

• | One-Piece Propeller Shaft Replacement

• | Two-Piece Propeller Shaft Replacement

• | Three-Piece Propeller Shaft Replacement

• | Four-Piece Propeller Shaft Replacement

6. Adjust the parking brake. Refer to Park Brake Adjustment .
7. Lower the rear wheel.
8. Remove the wheel blocks.