For 1990-2009 cars

### Removal Procedure

1. Remove the battery carrier cover.
2. Remove the terminal caps (3).

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

3. Disconnect the negative cables from the negative battery terminals (1).
4. Disconnect the positive cables from the positive battery terminals (4).
5. Remove the battery hold-down retainer nuts (3).
6. Remove the battery hold-down retainer (1) and cushion (7).
7. Remove the battery from the carrier.
8. Inspect the following components for damage:

8.1. | The batteries

8.2. | The cables and the connectors

8.3. | The carrier

9. Clean the components as necessary.

### Installation Procedure

1. Install the battery into the cleaned carrier.
2. Install the battery hold-down retainer (1) and cushion (7).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the hold-down retainer nuts (3).

Tighten
Tighten the hold-down retainer nuts to 17 N·m (13 lb ft).

4. Connect the positive cables to the positive battery terminals and install the nuts (2).

Tighten
Tighten the terminal nuts to 23 N·m (17 lb ft).

5. Connect the negative cables to the negative battery terminals and install the nuts (2).

Tighten
Tighten the terminal nuts to 23 N·m (17 lb ft).

6. Install the terminal caps (3).
7. Install the battery carrier cover.