For 1990-2009 cars

Cause | Action
--- | ---
DEFINITION: The clutch pedal requires high effort to operate. Review the Symptoms - Clutch and perform the necessary inspections.
Faulty clutch cable |

1. Inspect for the clutch cable and routing.
2. Route the cable for proper operation.
3. Replace the clutch cable if kinked, cut, or damaged. Refer to Clutch Cable Replacement .

Incorrect clutch cable return spring |

1. Inspect for the correct cable return spring.
2. Ensure the spring is properly installed. Refer to Clutch Release Arm Replacement .

Linkage requires lubrication | Perform the lubrication maintenance on the clutch linkage components.
Linkage interference |

1. Inspect for lines, hoses, or wiring harnesses interfering with the clutch linkage.
2. Repair the lines, hoses, or wiring harnesses away from the clutch linkage.

Linkage worn or damaged | Replace the faulty linkage components.
Clutch disc worn too thin | Replace the clutch assembly. Refer to Clutch Assembly Replacement .