For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cooling System

- 8.1L Engines - with manual transmission

25.0 L

26.5 qt

- 8.1L Engines - with automatic transmission with sloped hood

23.0 L

24.5 qt

- 8.1L Engines - with automatic transmission with specialty hood

25.0 L

26.5 qt

- 7.2L Engines - with manual transmission

30.0 L

32.0 qt

- 7.2L Engines - with automatic transmission

28.4 L

30.0 qt

Single-Speed Model - capacities are approximate

- 15040S EATON (H10)

10.0 L

10.5 qt

- S150-S DANA (H08)

11.6 L

12.3 qt

- R-160 ROCKWELL (H14)

19.0 L

20.0 qt

- 19060S EATON (HXB) (HPK) (HXC)

13.0 L

14.0 qt

- 19060D EATON (HPL)

13.0 L

14.0 qt

- 21060D EATON(HPN)

13.0 L

14.0 qt

- 21060S EATON (HPP)

13.0 L

14.0 qt

- 22060S EATON (HPG)

13.0 L

14.0 qt

- 23080S EATON (HPQ)

19.0 L

20.0 qt

- 23105S EATON (HNA)

26.5 L

28.0 qt

- 23431 EATON (HNG)

19.0 L

20.00 qt

- 26085P 26080P (HVQ)

19.0 L

20.0 qt

- 26105S EATON (HPA)

26.5 L

56.0 qt

- 30105S EATON (HPB)

25.5 L

28.0 qt

Tandem Models (capacities are approximate)

- DS344 EATON (HPI)

14.5 L

15.3 qt

- DS454P EATON (HPD)

14.5 L

15.3 qt

- DS404 EATON (HPE)

14.5 L

15.3 qt

- DS404P EATON (HPJ)

14.5 L

15.3 qt

- DD404P EATON (HXF)

14.5 L

15.3 qt

- DT402P EATON Rear Unit (HWU)

16.5 L

35.0 qt

Two-Speed - capacities are approximate

- 19050T EATON (H17)

15.5 L

16.4 qt

- 19060T EATON (HPM)

16.0 L

17.0 qt

- 21060T EATON (H15)

16.0 L

17.0 qt

- 22060T EATON (HPH)

16.0 L

17.0 qt

- 23080T EATON (H20)

19.0 L

20.0 qt

- 26080T EATON (GJ4)

19.0 L

20.0 qt

Engine Crankcase

- 8.1L Engine - with oil filter replacement

6.1 L

6.5 qt

- 8.1L Engine - without oil filter replacement

7.5 L

8.0 qt

- 7.2L Engine (with oil filter replacement)-Shallow

18.0 L

19.0 qt

- 7.2L Engine - with oil filter replacement - Deep

28.0 L

29.5 qt

- 7.2L Engine - overhaul - Shallow

21.0 L

22.0 qt

- 7.2L Engine - overhaul - Deep

32.0 L

34.0 qt

Fuel Tanks

- Standard Fuel Tank

189.0 L

50.0 gal

- Optional Fuel Tank

132.5 L

35.0 gal

- Optional Fuel Tank

227.1 L

60.0 gal

- Optional Dual 132 liter (35 gal) tanks

264.0 L

70.0 gal

- Optional Dual 189 liter (50 gal) tanks

378.0 L

100.0 gal

Transmission-Automatic

- AT545 ALLISON (MF1) Servicing-Shallow Pan *

8.5 L

9.0 qt

- AT545 ALLISON (MF1) Servicing-Deep Pan *

15.0 L

16.0 qt

- AT545 ALLISON (MF1) Rebuild/Dry-Shallow Pan *

14.0 L

15.0 qt

- AT545 ALLISON (MF1) Rebuild/Dry-Deep Pan *

21.0 L

22.0 qt

- MT643D ALLISON (ME3) Fluid and Filter *

11.0 L

12.0 qt

- MT643D ALLISON (ME3) Initial Fill After Rebuild *

20.0 L

21.0 qt

- MT643D ALLISON (ME3) Shallow Pan-Dry *

17.0 L

18.0 qt

- MT643D ALLISON (ME3) Deep Pan-Dry *

22.0 L

23.0 qt

- MT643G ALLISON (ME4)Fluid and Filter *

11.0 L

12.0 qt

- MT643G ALLISON (ME4) Initial Fill After Rebuild *

20.0 L

21.0 qt

- MT643G ALLISON (ME4) Shallow Pan-Dry *

17.0 L

18.0 qt

- MT643G ALLISON (ME4) Deep Pan-Dry *

22.0 L

23.0 qt

- 653DRG ALLISON (ME6) Fluid and Filter *

14.0 L

15.0 qt

- 653DRG ALLISON (ME6) Initial Fill After Rebuild *

20.0 L

21.0 qt

- 653DRG ALLISON (ME6) Shallow Pan-Dry *

17.0 L

18.0 qt

- 653DRG ALLISON (ME6) Deep Pan-Dry *

22.0 L

23.0 qt

- 653DRD ALLISON (ME5) Fluid and Filter *

14.0 L

15.0 qt

- 653DRD ALLISON (ME5) Initial Fill After Rebuild *

20.0 L

21.0 qt

- 653DRD ALLISON (ME5) Shallow Pan-Dry *

17.0 L

18.0 qt

- 653DRD ALLISON (ME5) Deep Pan-Dry *

22.0 L

23.0 qt

- MD3060P ALLISON (MNK) Fluid and Filter *

18.0 L

19.0 qt

- MD3060P ALLISON (MNK) Dry Fill *

22.0 L

23.0 qt

- MD3060P ALLISON (MP8) Fluid and Filter *

18.0 L

19.0 qt

- MD3060P ALLISON (MP8) Dry Fill *

22.0 L

23.0 qt

- MD3560P ALLISON (MNZ) Fluid and Filter *

18.0 L

19.0 qt

- MD3560P ALLISON (MNZ) Dry Fill *

22.0 L

23.0 qt

- MD3560P ALLISON (MTP) Fluid and Filter *

18.0 L

19.0 qt

- MD3560P ALLISON (MTP) Dry Fill *

22.0 L

23.0 qt

- LCT 2400 5 Spd. ALLISON (MTW) Shallow Pan *

12.0 L

13.0 qt

- LCT 2400 5 Spd. ALLISON (MTW) Standard Pan *

14.0 L

15.0 qt

- LCT 2400 5 Spd. ALLISON (MTW) Dry Fill *

18.0 L

19.0 qt

- LCT 2000 5 SPD AUTO ALLISON (MX4) Shallow Pan *

12.0 L

13.0 qt

- LCT 2000 5 SPD AUTO ALLISON (MX4) Standard Pan *

14.0 L

15.0 qt

- LCT 2000 5 SPD AUTO ALLISON (MX4) Dry Fill *

18.0 L

19.0 qt

Transmission-Manual

- FS6406A BOOS SYNC 6 SPD. EATON (MM8)

8.5 L

9.0 qt

- ES52-7B SPICER (MK8)

10.4 L

11.0 qt

- ES066-7B SPICER (MK9)

10.4 L

11.0 qt

- FS4205A 5-Speed EATON/FULLER (MSG)

4.5 L

5.0 qt

- FS4205B EATON/FULLER (MSC)

4.5 L

5.0 qt

- FS5205A 5-Speed EATON/FULLER (MPU)

5.0 L

5.3 qt

- FS5205C 5-Speed EATON (MNC)

5.9 L

6.2 qt

- FS5406A BOOS SYNC 6 SPD. EATON (MM7)

8.5 L

9.0 qt

- FS6305A 5-Speed FULLER (MKO)

9.0 L

9.5 qt

- FS6305B 5-Speed FULLER (MLO)

9.0 L

9.5 qt

- RT8908LL 10 SPD EATON (MT3)

13.2 L

14.0 qt

- RT6609 9-Speed FULLER (MUT)

5.7 L

6.0 qt

- FS08406 6 SPD. EATON (M69)

8.5 L

9.0 qt

- RT8709 9 SPD EATON (MS9)

12.3 L

13.0 qt

*Add 1.0 liter or 2.0 pints with spin-on filter.