For 1990-2009 cars

#### Tools Required

• | J 43764 Torque Converter End Play Gauge

• | J 5959 Dial Indicator Clamp and Adjuster

• | J 7872 Magnetic Base Dial Indicator

1. Position the torque converter (3) on the work table so that the pump hub is facing up.
2. Install J 43764 (2) into the torque converter hub.
3. Hold J 43764 (2) in the converter hub and rotate the center screw until J 43764 is locked into the converter hub. Do not over tighten J 43764 .
4. Assemble the following tools and install the tools onto the torque converter as shown:

• | J 5959 (1)

• | Extension rod (7)

• | Clamp (6)

• | J 7872 (4)

• | Adaptor rod (5)

5. Adjust the clamp (6) so that the dial indicator (1) firmly contacts the top of J 43764 (2).
6. Set the J 5959 (1) to read zero.
7. Lift J 43764 (2) upward as far as possible.
8. Read the J 5959 (1) to determine torque converter end play.
9. Compare the measured end play with the torque converter end play specifications. Refer to End Play Specifications .
10. If the measured torque converter end play exceeds the value listed, replace the torque converter.
11. Remove the J tools from the converter housing.