For 1990-2009 cars

### Removal Procedure

1. Place a suitable container under the hub cap in order to catch the oil.
2. Remove the bolts (1) and the washers (2).
3. Remove the hub cap (3) and the gasket (4). Do not allow gasket material to fall into the hub (10).

### Installation Procedure

1. Install a new gasket (4) and the hub cap (3) onto the hub (10). Align the gasket properly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts (1) and new washers (2).

Tighten
Tighten bolts evenly to 13 N·m (115 lb in).

3. Install new lubricant. Refer to Adding Lubricant to Hub Caps .