For 1990-2009 cars

#### Tools Required

J 43320 Crankshaft Rear Seal Puller

1. Install the J 43320 guide pins into the crankshaft.
2. Install the J 43320 over the guide pins.
3. Using a suitable drill, insert eight of the self-drilling sheet metal screws (1-8) into the rear crankshaft seal, using a criss-cross pattern. The self-drilling screws are included with the J 43320 .
4. Thread the center bolt of J 43320 into the crankshaft to remove the seal.
5. Remove the J 43320 guide pins from the crankshaft.