For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cast-Type Wheel Nut Final Torque | 271 N·m | 200 lb ft
Eight Hole, Aluminum or Steel Hub-Piloted Wheel Nut Final Torque | 550 N·m | 400 lb ft
Ten Hole, Aluminum or Steel Hub-Piloted Wheel Nut Final Torque | 644 N·m | 475 lb ft
Ten Hole, Aluminum or Steel Stud-Piloted Wheel Nut Final Torque | 644 N·m | 475 lb ft
Ten Hole, Steel Stud-Piloted Wheel and Stud Nut Final Torque | 800 N·m | 590 lb ft
Valve Stem Nut | 6 N·m | 53 lb in