For 1990-2009 cars

Application | Metric | English
--- | --- | ---
All Wheels (Except Dual Wheel Applications)

- Lateral Runout at the Rim

1.8 mm max.

0.07 in max.

- Lateral Runout at the Tire Edge

3.1 mm max.

0.125 in max.

Dual Wheel Applications

- Radial Runout at the Rim

3.1 mm max.

0.125 in max.

- Lateral Runout at the Rim

4.7 mm max.

0.187 in max.

- On-Vehicle Hub Check

2.3 mm max.

0.0938 in max.