For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 18 N·m | 13 lb ft
Bearing Retainer Bolts | 20 N·m | 15 lb ft
CSC Assembly | 20 N·m | 15 lb ft
Clutch Housing Cover Bolts | 22 N·m | 16 lb ft
Gear Shift Selector Rod Bush Securing Screw | 20 N·m | 15 lb ft
Locking Lever Spring Retainer | 60 N·m | 44 lb ft
Oil Drain and Fill Plug | 35 N·m | 26 lb ft
Quick Connect Attaching Bolt | 10 N·m | 89 lb in
Rear Bearing Plate | 10 N·m | 89 lb in
Rear Flange Nut | 100 N·m | 74 lb ft
Reverse Block Retaining Bolt | 10 N·m | 89 lb in
Reverse Idler Gear Shaft Locating Bolt | 25 N·m | 18 lb ft
Reverse Idler Gear Thrust Plate Retaining Bolt | 25 N·m | 18 lb ft
Shift Detent Spring Cover Bolt | 10 N·m | 89 lb in
Speed Sensor | 10 N·m | 89 lb in
Transmission-to-Engine Studs and Bolts | 60 N·m | 44 lb ft
Transmission Mounting Bolts | 50 N·m | 37 lb ft
Transmission Mounting Nuts | 45 N·m | 33 lb ft