For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Drag Link Ball Joint to Steering Arm Nut | 270 N·m | 200 lb ft
Draw Key Nut | 50 N·m | 37 lb ft
Engine Mount Nuts - Pass-through bolts | 70 N·m | 52 lb ft
Engine Mount Nuts - Except mount pass-through bolts | 85 N·m | 63 lb ft
Front Stabilizer Shaft Link Mounting Bolt Nut | 240 N·m | 177 lb ft
Front Stabilizer Shaft U-Bolt Nut | 24 N·m | 18 lb ft
Hub Cap Bolt | 13 N·m | 115 lb in
Hub to Drum Dayton-Walther, Nut

- 7/16-20

54 N·m

40 lb ft

- 1/2-20

90 N·m

66 lb ft

- 9/16-18

110 N·m

81 lb ft

- 5/8-18

151 N·m

110 lb ft

- 3/4-16

300 N·m

221 lb ft

Hub to Rotor Bolt

- 1/2-20

120 N·m

88 lb ft

- 5/8-11

225 N·m

166 lb ft

- 9/16-12

163 N·m

120 lb ft

King Pin Cap Bolt - Except FH4 | 24 N·m | 18 lb ft
King Pin Cap Bolt - With FH4 | 35 N·m | 26 lb ft
King Pin Nut | 550 N·m | 406 lb ft
Shock Absorber, Lower Nut | 84 N·m | 62 lb ft
Shock Absorber, Upper Nut | 84 N·m | 62 lb ft
Spring Bumper Mounting Nut | 68 N·m | 50 lb ft
Spring Bumper Stop Nut | 40 N·m | 30 lb ft
Spring Eye Bolt | 330 N·m | 243 lb ft
Spring Hanger Nuts | 85 N·m | 63 lb ft
Tie Rod Ball Joint Nut - With FH4 | 268 N·m | 198 lb ft
U-Bolt Nut - FL1 Axles | 225 N·m | 166 lb ft
U-Bolt Nut - Except FL1 Axles | 425 N·m | 314 lb ft