For 1990-2009 cars

### Removal Procedure

1. Remove the bolt from the tail lamp.
2. Remove the tail lamp.
3. Remove the electrical connector from the tail lamp

### Installation Procedure

1. Install the tail lamp. Align the locator with the hole in the frame rail.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolt into the tail lamp. Make sure that the harness retaining clip is secured by the bolt.

Tighten
Tighten the tail lamp bolt to 35 N·m (26 lb ft).

3. Connect the electrical connector to the tail lamp.