For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle with safety stands. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove engine cover to gain access to rear mounts. Refer to Engine Cover Replacement in Interior Trim.
3. Support the engine using suitable safety stands.
4. Disconnect any engine harness clips or line routing on the engine mount bracket.
5. Use a suitable engine hoist to lift weight off the engine mounts.
6. Remove the engine rear mount bracket to engine mount.
7. Remove the rear engine mount bracket. Refer to Engine Rear Mount Bracket Replacement .
8. If the body mount is supported by the engine mount fasteners support the body with a jack or stand.
9. Remove the engine mount to frame bolts/nuts.
10. Remove the rear engine mount assembly.

### Installation Procedure

1. Install the rear engine mount assembly.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear engine mount to frame nuts
3. Install the engine mount to frame nuts.

Tighten
Tighten the rear engine mount to frame nuts to 160 N·m (118 lb ft).

4. Install the rear engine mount bracket. Refer to Engine Rear Mount Bracket Replacement .
5. Remove jacks or stands supporting the body if used.
6. Lower the rear engine mount bracket on to the engine mount.
7. Install the rear engine mount bracket to engine mount nut.

Tighten
Tighten the rear engine mount bracket to the engine mount nut to 195 N·m (144 lb ft).

8. Install any engine harness clips or lines routing on the engine mounts.
9. Remove the engine safety stands and engine hoist.
10. Install engine cover. Refer to Engine Cover Replacement in Interior Trim.
11. Lower the vehicle.