For 1990-2009 cars

#### Tools Required

• | J 44529 Stator Shaft Bushing Remover

• | J 8092 Universal Driver

• | J 43774 Stator Shaft Bushing Installer

Notice: Always use J 44529 when removing the stator shaft bushing to help avoid damage to the stator shaft sealing surface.

1. Position the oil pump cover assembly (10) supported by wooden blocks with the stator shaft facing up.
2. Install J 44529 -2 bolt (8) into J 44529 -1 extractor (7).
3. Install J 44529 -2 bolt (8) and J 44529 -1 extractor (7) into the bushing (9).
4. Install washer (6) and nut (5) onto J 44529 -2 bolt (8).
5. Hold the top of J 44529 -2 bolt (8) with a wrench and tighten nut (5) until J 44529 -1 extractor (7) engages the bushing (9).
6. Install J 44529 -3 protector (4) onto J 44529 -2 bolt (8) .
7. Install bearing (3), washer (2), and nut (1) onto J 44529-2 bolt (8).
8. Hold the top of J 44529 -2 bolt (8) with a wrench and tighten nut (1) until the bushing is dislodged.
9. Remove the J tools from the stator shaft.
10. Remove the bushing from the J tools.

Important: The preferred method for installing the stator shaft bushing is to use J 43774 and a press. If a press is not available, use J 43774 and J 8092 universal driver. If the bushing will be installed without a press, install the large end of J 43774 (2) onto J 8092 (1).

11. Install a new bushing (3) onto J 43774 .
12. Drive the bushing into the stator shaft (4) until the bushing is seated.

Specification
The bushing installed depth measurement is flush to 0.25 mm (0.010 in) below the stator shaft surface.