For 1990-2009 cars

Important: Mark, organize and sort the cylinder head components. Return the components to their original location during reassembly. Make an organizer rack from a piece of wood.

1. Remove the valve rocker arm nuts, the valve rocker arm balls and the valve rocker arms.

Important: The exhaust valve push rods (2) are longer than the intake valve push rods (1).

2. Remove the valve push rods.
3. Remove the valve rocker arm studs and push rod guides.